EECS 3150

Data Communication

Project 1

Milestone 1

J Andrew McCormick

10/8/2015

**Table of Contents**

How to Run ……………………………………………………………………………………… 1

**How to Run**

In order to run this program, you must follow the following steps:

1. Using two terminal windows, navigate to the root directory in each window.

2. Run make from the root directory (where the makefile is located).

3. In one of the windows type ./rcvr and press enter (this will open up the receiver where it waits for something to be transmitted) (the receiver and transmitter operate on the localhost at port 5050).

4. In the other window, type ./xmtr and press enter.